# Software Information
display_name = "Sinclair - ZX Spectrum (Fuse)"
authors = "Team Fuse"
supported_extensions = "tzx|tap|z80|rzx|scl|trd|dsk|dck|sna|szx|zip|ipf"
corename = "Fuse"
categories = "Emulator"
license = "GPLv3"
permissions = ""
display_version = "1.6.0"

# Hardware Information
manufacturer = "Sinclair|Amstrad"
systemname = "ZX Spectrum (various)"
systemid = "zx_spectrum"

# Libretro Features
supports_no_game = "true"
database = "Sinclair - ZX Spectrum +3|Sinclair - ZX Spectrum"

# BIOS / Firmware
firmware_count = 8
firmware0_desc = "128p-0.rom (Pentagon machines)"
firmware0_path = "fuse/128p-0.rom"
firmware0_opt = "true"
firmware1_desc = "128p-1.rom (Pentagon machines)"
firmware1_path = "fuse/128p-1.rom"
firmware1_opt = "true"
firmware2_desc = "trdos.rom (Pentagon machines)"
firmware2_path = "fuse/trdos.rom"
firmware2_opt = "true"
firmware3_desc = "gluck.rom (Pentagon 512K / 1024)"
firmware3_path = "fuse/gluck.rom"
firmware3_opt = "true"
firmware4_desc = "256s-0.rom (Scorpion 256K)"
firmware4_path = "fuse/256s-0.rom"
firmware4_opt = "true"
firmware5_desc = "256s-1.rom (Scorpion 256K)"
firmware5_path = "fuse/256s-1.rom"
firmware5_opt = "true"
firmware6_desc = "256s-2.rom (Scorpion 256K)"
firmware6_path = "fuse/256s-2.rom"
firmware6_opt = "true"
firmware7_desc = "256s-3.rom (Scorpion 256K)"
firmware7_path = "fuse/256s-3.rom"
firmware7_opt = "true"
notes = "[1] Amstrad have kindly given their permission for the redistribution|[^] of their copyrighted material but retain that copyright."

description = "A port of the Fuse Unix Spectrum Emulator to libretro, this core supports many Spectrum, Timex, Pentagon and Scorpion variants. The Pentagon and Scorpion machines need BIOS images placed inside a 'fuse' subdirectory inside the frontend's 'system' directory. This core is a good first choice for playing Spectrum games, with 81 (EightyOne) covering the Sinclair ZX 81 games."
